                           0 10 20 30 40

         50

   100

   150

   200

Data Size (kB)

Frequency (Hz)

Required Limit (500/6 = 83Hz)

Xfer Speed of the Belle DAQ System

Measured (by Matsuo)

25-Nov-1997 by H.Fujii